Very simple and therefore very fast examples. No heavy libraries, but just two functions.

There are two examples, one for 12/14/16 bit resolution and one for 18 bit resolution.

Code was tested on Arduino, Nano, ESP32, Maple and NUCLEO F411.